Glossaire



|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
| AAM | *Air to Air Missile* |
| AMRAAM | *Advanced Medium Range Air to Air Missile* |
| BARCAP | *Barrier Combat Air Patrol* |
| BRAA | *Bearing Range Altitude Aspect* |
| BRT | *Brightness* |
| BVR | *Beyond Visual Range* |
| CAC | *Close Air Combat* |
| CAP | *Combat Air Patrol* |
| CCIP | *Continuously Computed Impact Point* |
| CCRP | *Continuously Computed Release Point* |
| CON | *Contrast* |
| DCLT | *Declutter* |
| DED | *Data Entry Display* |
| DGFT | *DoG FighT* |
| DTE | *Data Transfer Equipment* |
| DTOS | *Dive TOSs* |
| EEGS | *Enhanced Envelope Gun Sight* |
| FCR | *Fire Control Radar* |
| FLCS | *Flight Command System* |
| FLIR | *Forward Looking InfraRed* |
| GAN | *Gain* |
| GCI | *Ground Control Interception* |
| HAD | *Harm Attack Display* |
| HARM | *High-speed, Anti-Radiation*Missile |
| HSD | *Horizontal Situation Display* |
| HUD | *Head Up Display* |
| INV | *Inventory* |
| LADD | *Low Altitude Drogue Delivery* |
| MAU | *Type d’ejector Rack » pour arme conventionnelle et Réservoir,* |
| MFCD | *Multi Functions Color Display* |
| MFD | *Multi Functions Display* |
| MRL | *Missile Rail Launcher,* |
| NSTL | *NoSe TaiL* |
| OSB | *Option Select Button,* |
| RNG | *RaNGe* |
| RP | *Release Pulse* |
| RWR | *RADAR Warning Receiver* |
| RWS | *Range While Search* |
| SA | *Situation Awarness* |
| SAM | *Situational Awareness Mode* |
| SEAD | *Suppression of Enemy Air Defenses* |
| SGL | *SiNgLe* |
| SITAC | *SITuation TACtique* |
| SITAC | *Situation Tactique* |
| S-J | *Selective Jettison,* |
| SMS | *Store Management System* |
| STRF | *Strafe,* |
| STT | *Single Target Track* |
| SYM | *Symbology* |
| TARCAP | *TARget Combat Air Patrol* |
| TER | *Triple Ejector Rack* |
| TFR | *Terrain Following Radar* |
| TGP | *TarGeting Pod* |
| TWS | *Track While Scan* |
| WP | *WayPoint* |
| WPN | *WeaPoN* |